### Test 060-16-03 SCS Re-key

#### Description

##### PD

Confirm there is a process to remove the paired key from a PD.

##### ACU

Confirm that an ACU can cease using a paired key with a given PD.

#### Purpose

Show the paired secure channel key can be disposed of.

#### Criteria

|  |  |
| --- | --- |
| Basic OSDP (PD) | Optional |
| Basic OSDP (ACU) | Optional |
| Secure Channel (PD) | Required |
| Secure Channel (ACU) | Required |
| BIO Match (PD) | Required |
| BIO Match (ACU) | Required |
| BIO Read (PD) | Required |
| BIO Read (ACU) | Required |
| Extended Packet Mode (PD) | Required |
| Extended Packet Mode (ACU) | Required |
| Extended Read/Write (PD) | Optional |
| Extended Read/Write (ACU) | Optional |

#### Test action

##### PD Test

Un-pair the PD.

##### ACU Test

Induce the ACU to forget the current paired key and return to install mode.

#### Development status

Available in libosdp-conformance 1.28-2

#### Test Results

JSON tags

|  |  |
| --- | --- |
| test | 060-12-03 |
| test-status | 1 for pass, 0 for fail |

#### Revision History

Refreshed for 2.1.